V12 DDS upgrade operation instruction:
1, open the firmware program
2, connect the steering wheel to the computer via USB-B cable.
3, when the program shows that "the device is connected(设备已连接)“, click the ”update(更新)“ button



