PXN-V99 Steering Wheel Firmware V0.67

Update Instructions:

1, Open the firmware update software.
2, Press and hold the “HOME” button in the center of the wheel, then connect the steering wheel's USB cable to the computer.
3, Once the software displays "Device Connected" , release the HOME button.
4, Click "Update" to begin the firmware update process.
5, When a pop-up window displays "Update is Successful", the update is complete.
Note: During the update process, do not disconnect the steering wheel from the computer.

If you have further questions, please contact the PXN Support Team at support@e-pxn.com.

